**TinyG Data Sheet Version 8**

Pat Farrell edited this page on Feb 6, 2014 · [1 revision](https://github.com/synthetos/TinyG/wiki/Data-Sheet---Version-8/_history)

Draft mockup. None of these numbers are real, yet.

This is the specification data sheet for the TinyG version 8 board. All specifications are subject to change as we improve the product.

version

8

release date:

2013

board physical size

20mm w by 30 mm long by 12 mm high. Note, any board enclosure must provide adequate cooling.

Number of motors supported

4

chaining/networking multiple TinyG together to support additional numbers of motors

Yes

maximum current per motor

3 amps

maximum voltage to motors

30 volts DC

spindle speed control

yes, using PWM output

https://github.com/synthetos/TinyG/wiki/Data-Sheet---Version-8